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BU-P5223-@
(Triaxial Cable Assembly, Male Both Ends)
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· BU-P5223 is a triaxial cable assembly with a male BNC connector at each end.
· Made with a Belden 9222 double shielded triaxial cable for use in high interference areas.
· Material:	Triaxial cable male		BNC, 3 lug bayonet style
Finish				Tarnish-resistant brass
Center contacts		Gold-plated
Cable	insulation		Polyethylene
· Ratings:	Operating Voltage		500 VRMS/DC
Impedance, cable		50 Ohms
· The “@” in the model number represents the overall length in inches. Standard lengths are: 36”, 60”
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